~~REVEAL theme=laser_cutter_preflight&transition=fade&controls=0&show_progress_bar=1&build_all_lists=0&open_in_new_window=0~~

Laser Cutter Checks

The Edge standard checks for the Rayjet 300.

Laser Cutter Preflight Checks - Prepare Your Job

Hot Work Permit active

Material purchased, checked by supervisor

Honeycomb correctly seated on bed

Focal distance correctly calibrated to stock

Starting position of laser is correct

Laser Cutter Preflight Checks - Supervisor Check

Starting position of laser is correct - verified by Supervisor

Bed is correctly seated - verified by Supervisor

Focus alignment - verified by Supervisor

All cut settings - verified by Supervisor

power

speed

number of passes

Auto focus feature disabled - verified by Supervisor

Update Settings, apply and press OK

Laser Cutter Checks - During Cut

Start job from Laser Cutter NOT software

Avoid looking directly at the laser flash

Prolonged exposure to laser flash may cause eye strain

Abort job if material catches fire

ALERT SUPERVISOR

Pause Job to adjust

ALERT SUPERVISOR

repeat pre-flight check if needed

Laser Cutter Checks - After Cut

Wait 30 secs for fumes to clear

Remove Job

Brush out or vacuum debris

Laser Cutter Checks - After Session

Leave area clean and tidy

Take your USB

Show of your work on made today