Multicam CNC Staff Operations Signage

Daily Setup

Prepare Space

20160922_103719.jpg

Sign out Pit Key

Establish Comms via walkie talkie (Channel 21)

Open Roller Door

Place bollards out for CNC work area

Check dust extractor bag /Empty if required

Prepare Space Continued

Turn on compressor

Ensure required PPE is available and that the space is tidy enough to commence work.

Remove MDF cover board from waste board.(2 person lift recommended)

Check the condition of waste board for high spots and lightly sand where necessary

Turn on the CAD Computer, digital signage, lights and fan where necessary

Setup Machine

If there is a cutting tool/bit on the machine - ensure it is secure.

Ensure Spindle is clear for warmup procedure.

Test Vacuum Bed Compressor

Test Dust Extractor

Setup Machine Continued

Turn on CNC machine and wait for it so go through its start up procedure

Home the machine

select Warm up spindle and OK (5 Mins)

Daily Machine Pack Down

Cleaning up

Throw away any off-cuts or larger debris

Use extraction tube to vacuum the material before removing, once removed vacuum the waste board. Use the dust pan to remove any debris still stuck on the board by scraping it off lightly.

Use compressed air clean around and underneath the machine.

Use compressor to clean the machine, most importantly the linear rails.

Replace Night Cover on Wasteboard

Return tools to tool storage

Tidy up work bench (dust, wipe if needed)

Make sure space is tidy for next person to use

Bring the barriers back in, shut the door and turn off the light

Shutting Down

Return the Machine to Home position

Turn off machine by pressing the Off button

Turn off Vacuum bed and Extraction fan on the wall

Shutdown CAD Computer via Windows menu

Turn off Monitor, Fan, Lights, Compressor and WAP

LINKS CNC Router Operations Other Operations - Staff Only Multicam CNC Induction

facilities:fablab:equipment-cots:multicam_m-2412:Supervisor preflight check}}