Main parts on CNC machine

Machine bed - with vacuum suction

Steel Gantry - X axis

Machine head - Y and Z axis

Spindle - routing bits and collets spins at 16000rpm average

Controller panel - Manually control the gantry and load jobs

Inverter enclosure- DO NOT OPEN! High Voltage. Main on/off switch is located here.

Vacuum Pump manifold - four sections can be isolated to increase vacuum.