Pausing a Cut / Clearing Debris

If a piece is moving or get stuck in the extractor.

Pause the cut with the red stop button

Wait for the machine head to withdraw

Watch the controller

Wait for the spindle to stop

Watch the spindle - verify it has stopped.

Use emergency stop if necessary

Note -if the machine is turned OFF mid operation, wait 1 minute to turn ON.