Planeing the Wasteboard

1) Position the wasteboard hard into the corner and location blocks

2) Turn on the vacuum pump!

3) Remove location blocks!!!`

For a new board both sides need to be dressed to remove wax coating and level the board. 1.5 to 2 months under heavy use. 1mm deep initially on first side on a fresh board .5mm deep on second side on a fresh board From this point the board should need not flipped until a new board is used. .2mm deep there after on the same side

Planning the Wasteboard

4) Key in F28 on A2MC Console

Set waste board No

Wasteboard must be set AFTER the planing table or machine bed damage may result!

Plane table yes

Tool Diameter 45

Overlap 50%

Length (X Axis) 2420mm

Width (Y Axis) 1230mm

Z depth .5 mm

Feed rate 12000mm

Spindle RPM 10000

Set origin NO

Plane table Yes

Set the Wasteboard

When planing is complete replace location blocks.

Now you need to set the waste board (ie zero the Z Axis)

5) Key in F28 on A2MC Console

Set waste board Yes

Jog tool down to complete a manual tip off (as per manual tip off) and press OK when you are have just touched.

LINKS CNC Router Operations Other Operations - Staff Only Multicam CNC Induction