LFA Case Version 1.0

Case Design

Components

Pelican iM2875 case

Custom Foam insert

8 * 500mm power cables

8 Socket powerboard

8 * Lindy USB power chargers

Assembly

Grab the 500mm power leads and coil up until you have about 50mm of play at each end, then cable tie tight.

Slide the first PSU in the top slot

Flip the foam round and plug-in the first power-cable

Repeat for the remaining cables

Plug in all the cables to the powerboard

Wedge the powerboard into the bottom of the foam - make sure the powerboard lead is fed up through the hole.

Fit the foam in the case

Files

Current

Fusion360 Model

IGS (IGS format)

Old

Original Foam Cutting files (IGS format)