Shut down

Make sure the machine is clear of any tooling.

Press 'Reset' then 'Home' to realign machine to zero.

Remove tooling and collet, put away.

Send machine to 'safe' posision.

Press 'STOP!' button.

Put away tools, PPE and scrap material

Vaccume and sweep up workspace.