CNC Pit Setup

OH&S dictates that the CNC Pit needs to remain tidy. For some time there will be weekly inductions ( 5 participants plus facilitator) and open lab access ( min 2 people)

To achieve this we will have a specifc list of furniture and equipment stored there. Anything else needs to be removed be the machine is used.

Tools

Battery drill and charger

Phillips head Driver bit

Drill bits

Screws and washers ( well labeled so bed is never punched with longer screws )

Mallet

Water spray

Chuck Wrench 1

Chuck wrench 2

Tape measure

Veneer calliper

Multi Cam Manual

Tooling/ collets

Tarp

Stationary

Markers (sharpie)

Pencil

Whiteboard markers

Biro

Clipboards x 6

Broom

Cleaning/Maintenance

Spray and Wipe

Supply of Chux

WD40

Steel Wool

PPE

Gloves ( for changing tool and manual handling) x 6 pairs (C)

Eyes Protection Clean x 6 pairs (C)

Container Eyes Protection Worn (C)

Disposable Hearing protection(C)

Hearing protection (Muff type) (C)

Dust masks disposable (C)

Furniture

Whiteboard

6x stools

Bin ( no offcuts )

Computer bench

Bookshelves

Signage

(even if these are printouts initially)

Operator only inside line when machine is cutting

Line

Eye and hearing protection to be worn when machine is in operation

Cut settings

Right tool for the job

*(C)** A Stock of accountable consumables will be kept in the consumables store and will be stocktaked weekly. See Stock Control for procedures around these items.