Commonly Used Tabs and Functions

A2MC Tabs

FUNCTION	NOTES
Tab 1 - Jobs Mode
Tab 2 - Position & Jog Mode
Tab 3 - Speed Mode
Tab 4 - Spindle RPM
Tab 5 - Origin Mode
Tab 6 - Tooling Mode
Tab 7 - Function Mode

Spindle Functions

FUNCTION	NOTES
Function 01 - Machine Properties
Function 02 - Verify Job
Function 09 - Abort Job
Function 16 - Set Parking Position
Function 20 - Set Material Thickness
Function 25 - Set Tool Height
Function 27 - Set User Z Origin
Function 28 - Set and Plane Waste Board
Function 30 - Edit Tools
Function 31 - Change Active Tool
Function 40 - Current Job Properties
Function 41 - Feed Speed
Function 42 - Spindle Control
Function 43 - Job Repeat
Function 44 - Job Array
Function 45 - Plunge Speed
Function 46 - Measured Move
Function 47 - Cut Rectangle

Tangential Knife Functions

Function 24 - Set Knife Length
Function 42 - Rotate Knife
Function 58 - Swap from Spindle to Knife Control
Function 67 - Knife Overcut/Undercut Compensation
Function 822- Set up Tangential Knifes

LINKS CNC Router Operations Other Operations - Staff Only Multicam CNC Induction