Daily Machine Pack Down

Cleaning up

Throw away any off-cuts or larger debris

Use extraction tube to vacuum the material before removing, once removed vacuum the waste board. Use the dust pan to remove any debris still stuck on the board by scraping it off lightly.

Use compressed air clean around and underneath the machine.

Use compressor to clean the machine, most importantly the linear rails.

Replace Night Cover on Wasteboard

Return tools to tool storage

Tidy up work bench (dust, wipe if needed)

Make sure space is tidy for next person to use

Bring the barriers back in, shut the door and turn off the light

Shutting Down

Return the Machine to Home position

Turn off machine by pressing the Off button

Turn off Vacuum bed and Extraction fan on the wall

Shutdown CAD Computer via Windows menu

Turn off Monitor, Fan, Lights, Compressor and WAP

LINKS CNC Router Operations Other Operations - Staff Only Multicam CNC Induction