~~REVEAL~~

Daily Setup

Prepare Space

20160922_103719.jpg

Sign out Pit Key

Establish Comms via walkie talkie (Channel 21)

Open Roller Door

Place bollards out for CNC work area

Check dust extractor bag /Empty if required

Prepare Space Continued

Turn on compressor

Ensure required PPE is available and that the space is tidy enough to commence work.

Remove MDF cover board from waste board.(2 person lift recommended)

Check the condition of waste board for high spots and lightly sand where necessary

Turn on the CAD Computer, digital signage, lights and fan where necessary

Setup Machine

If there is a cutting tool/bit on the machine - ensure it is secure.

Ensure Spindle is clear for warmup procedure.

Test Vacuum Bed Compressor

Test Dust Extractor

Setup Machine Continued

Turn on CNC machine and wait for it so go through its start up procedure

Home the machine

select Warm up spindle and OK (5 Mins)