Multicam M-2412

CNC Router is a computer controlled version of the handheld router. It is used for cutting and hollowing shapes in hard materials - timber, plastics, aluminum. The CNC (computer numeric controlled) allows this machine to cut precise, repeatable, quick and efficient copies of a design.

The Edge's M-2412 is manufactured locally in Brisbane by Multicam CNC and features: A2MC Controller ELTE COLLET ER32 - 3HP Spindle with max speed of 18000RPM Multicam Oscillating Knife Vacuum Machine Bed Multicam Vision System 5 hp Dust Extractor Donek Drag knife and creaser

Other Upgrades Available

Tangential Knife

Pneumatic Tool Changer

Mist Sprayer

Parts of the machine

CNC Safety

~~REVEAL~~

CNC Router Operations

The Edge has developed a CNC Router Operations e-manual in order to safely and efficiently promote public engagement with this piece of equipment.

→ Read more...

Design to Cut

This page covers all the methods currently used and endorsed for use on the CNC. Each flow goes through:

Design - where shapes are generated

Preparation for Cutting

NC (numerical code) generation

In some workflows, this may involve two or more software applications. For example - DXF files generated in Illustrator may need to be modified or re-exported from Corel Draw or Fusion360. To test or recommend workflows, please use the CAM Software Testing page.

my_postp.zip

tool database

LINKS CNC Router Operations Other Operations - Staff Only Multicam CNC Induction