Daily Setup

Switch on power supply

Check that Flexible Steel Print Sheet is clean and damage free

Run Daily Setup Check script (found in the testing folder on the SD card) this will run a Z axis calibration extrude and print a small test print.

This is an operation for Level 2 inductees and above only