Supported Filaments

Common

PLA

Polylactic acid (Starch based)

ABS

Acrlonitrile butadiene styrene

ASA

PET

Polyethylene terephthalate (Glycol modified)

T-Glass (Taulman)

Nylon

Polyamide (Taulman Bridge)

HIPS

High-impact polystyrene

PVA

Polyvinyl acetate (Water-soluble Print support)

BVOH

PP

Polypropylene

Specialized

Composite Materials

Often PLA with carbon fiber, metal or wood fill

PC-ABS

(E3D) ABS Polycarbonate blend

PP

Polypropylene

Others

CPE (copolyester)
XT (ColourFabb)
HT (ColourFabb)	Amphora copolyester
nGen